Tutorial voor Cisco OSPF!!

Eerst dit lezen:

https://community.cisco.com/t5/networking-knowledge-base/understanding-passive-interface-default-command-in-ospf/ta-p/3120648

Welkom ! Deze zelfstudie geeft u een eenvoudige handleiding voor het configureren van basis- OSPF op een Cisco-router. Maar voordat we gaan configureren, laten we een overzicht hebben van OSPF.

**Over OSPF**

Open Shortest Path First (OSPF) is een van de dynamische routeringsprotocollen, waaronder  **EIGRP** , **BGP** en **RIP** . Het is misschien wel een van de meest populaire routeringsprotocollen voor **verbindingsstatussen .**Het is een open standaard, dus het kan worden uitgevoerd op routers van verschillende leveranciers.

OSPF ondersteunt **belangrijke functies** zoals:

* IPv4- en IPv6-routing
* Klasseloze routering
* Gelijke kosten load balancing,
* Handmatige routesamenvatting, enz.

OSPF has a default administrative distance of 110. It uses *cost* as the parameter for determining  route metric. It uses the multicast address of 224.0.0.5 and 224.0.0.6 for communication between OSPF-enabled neighbors

Routers running OSPF need to establish a neighbor relationship before exchanging routing updates. Each OSPF router runs the SFP algorithm to calculate the best routes and adds them to the routing table.

OSPF routers store routing and topology information in three tables.:

* ***Neighbor table***-which stores information about OSPF neighbors.
* ***Topology table***-stores topology structure of the network.
* ***Routing table***-stores the best routes

**OSPF neighborhood discovery**

Routers running OSPF need to establish a neighbor relationship before exchanging routing updates. OSPF neighbors are dynamically discovered by sending Hello packets out each OSPF-enabled interface on a router. Hello packets are sent to the multicast address of 224.0.0.5.

**OSPF areas**

An area is simply a logical grouping of adjacent networks and routers. All routers in the same area have the same topology table and don’t know about routers in other areas. The main benefits of using *areas* in an OSPF network are:

* Routing tables on the routers are reduced.
* Routing updates are reduced.

Each area in an OSPF network must be connected to the **backbone** **area** ( also known as ***area 0***). All routers inside an area must have the **same area ID***.*

A router that has interfaces in more than one area (for example area 0 and area 1) is known as an Area Border Router (**ABR**).  A router that connects an OSPF network to other routing networks (for example, to an EIGRP network) is called an Autonomous System Border Router (**ASBR**).

For now we’ll configure basic OSPF. On to it then!

**Basic  OSPF configuration.**

1. Build the network topology.

Afbeelding met tekst, diagram, lijn, schermopname

Automatisch gegenereerde beschrijving

Advertisements

REPORT THIS ADPRIVACY

2.Configure IP addresses on PCs and router interfaces.

**Router 1**

R1(config)#int fa 0/0

R1(config-if)#ip add 10.0.0.1 255.0.0.0

R1(config-if)#no shut

R1(config-if)#

R1(config-if)#int serial 0/0/0

R1(config-if)#ip add 20.0.0.1 255.0.0.0

R1(config-if)#no shut

**Router 2**

R2(config-if)#int fa0/0

R2(config-if)#ip add 30.0.0.1 255.0.0.0

R2(config-if)#no shut

R2(config-if)#

R2(config-if)#int serial0/0/0

R2(config-if)#ip address 20.0.0.2 255.0.0.0

R2(config-if)#no shut

Now do IP configurations for the PCs.

**PC1**  IP add 10.0.0.2  Subnet mask 255.0.0.0   Default gateway  10.0.0.1

**PC2** IP add 30.0.0.2  Subnet mask 255.0.0.0    Default gateway   30.0.0.1

Advertisements

REPORT THIS ADPRIVACY

3**. Configure OSPF** on the routers.

The configuration is pretty simple and requires only two major steps:

1.  Enable OSPF on a router using the *router* *ospf PROCESS\_ID* in the global configuration mode.

2.Define on which interfaces OSPF will run and what networks will be advertised using *network IP\_ADDRESS  WILCARD\_MASK  AREA*command in the OSPF configuration mode.

Note that the OSPF **process ID** *doesn’t have to be the same* on all routers in order for the routers to establish a neighbor relationship, but the **area** parameter *has to be the same* on all neighboring routers in order for the routers to become neighbors.

**Router 1**

R1(config)#

R1(config)#router ospf 1

R1(config-router)#network 10.0.0.0  0.255.255.255  area 0

R1(config-router)#network 20.0.0.0  0.255.255.255  area 0

**Router 2**

R2(config)#

R2(config)#router ospf  2

R2(config-router)#network 20.0.0.0  0.255.255.255 area 0

R2(config-router)#network 30.0.0.0  0.255.255.255 area 0

Advertisements

REPORT THIS ADPRIVACY

As you can see from the above picture,we just need to **enable OSPF** on the routers which then advertise the networks **directly connected** to each of them.

*Have in mind:*The **OSPF process IDs** used for the two routers  have been made **optionally** different but their **area  numbers** **must be** the same.

4. Verify OSPF configuration

First, let’s verify that the routers have established a neighbor relationship by typing the *show ip ospf neighbor*command on **R1**:

Afbeelding met tekst, schermopname, Lettertype, lijn

Automatisch gegenereerde beschrijving

Next, to verify that R1 has learnt the route to 30.0.0.0/8 network, we’ll use  *show ip route ospf* command on **R1**:



Note that the letter **O**indicates OSPF routes.

Lastly, verify connectivity. Ping **PC2** from **PC1**. Ping should be successful.

Afbeelding met tekst, software, computer, Webpagina

Automatisch gegenereerde beschrijving